Transmittal Report:

Created by AutoCAD eTransmit Tuesday, May 15, 2018, 1:57 PM.



Drawing:

This is a transmittal based on P07 Belgard PICP to Asphalt.dwg.



Files:



Root Drawing:

	P07 Belgard PICP to Asphalt.dwg



JPG File References:

	Belgard_logo_crop.jpg



AutoCAD Color-dependent Plot Style Table File References:

	BLG.ctb



AutoCAD Plotter Configuration File References:

	AutoCAD PDF (General Documentation).pc3



The following files were excluded from the transmittal:

	acad.fmp

	simplex.shx

	arial.ttf

	ltypeshp.shx

	calibri.ttf

	AWS.ctb





Conversion:

All drawing files were converted to AutoCAD 2013/LT 2013 format.





Notes for distribution:



Raster image files:

Image paths were removed, so all image files must be placed on the AutoCAD search path, a project search path or in the same directory as the root drawing.



.PC3 printer configuration files:

Please copy these files to the AutoCAD Printer Configuration Search Path directory.



.CTB/.STB plot style tables:

Please copy these files to the AutoCAD Plot Style Table Search Path directory.



The AutoCAD variable FONTALT was set to:

E:\p2c drive\_projects\cad standards\_p2c cad\support\simplex.shx

Please make sure that the FONTALT variable is set to this file or an equivalent before opening any drawings.  All text styles with missing fonts are automatically set to this font.







*** Map 2007 Data and Cache files ***



The drawing 'E:\P2C Drive\_Belgard\_Details\02 PICP\z Details\Finals\P07 Belgard PICP to Asphalt.dwg' refers to a cache manifest XML file, zero or more cache files (.GWS) as well as raw data files.

Please ensure the manifest XML file and cache files are unzipped to the drawing directory or your current MapCache directory.

You may also need to update the cache manifest XML file to point to the unzipped location of the data files.



