Transmittal Report:

Created by AutoCAD eTransmit Friday, February 15, 2019, 11:17 AM.



Drawing:

This is a transmittal based on S13 Belgard Std Paver Install Utility Str.dwg.



Files:



Root Drawing:

	S13 Belgard Std Paver Install Utility Str.dwg



JPG File References:

	Belgard_logo_crop.jpg



AutoCAD Color-dependent Plot Style Table File References:

	PlotCfgs\BLG.ctb

	PlotCfgs\AWS.ctb



AutoCAD Plotter Configuration File References:

	PlotCfgs\AutoCAD PDF (General Documentation).pc3



The following files were excluded from the transmittal:

	acad.fmp

	Fonts\simplex.shx

	Fonts\arial.ttf

	Fonts\calibri.ttf

	Fonts\ltypeshp.shx





Notes for distribution:



Raster image files:

Paths may be present on references to raster images.  Make sure these paths work or that the root drawing is using the correct references.



.PC3 printer configuration files:

Please copy these files to the AutoCAD Printer Configuration Search Path directory.



.CTB/.STB plot style tables:

Please copy these files to the AutoCAD Plot Style Table Search Path directory.



The AutoCAD variable FONTALT was set to:

E:\P2C Drive\_PROJECTS\CAD Standards\_P2C CAD\Support\simplex.shx

Please make sure that the FONTALT variable is set to this file or an equivalent before opening any drawings.  All text styles with missing fonts are automatically set to this font.







*** Map 2007 Data and Cache files ***



The drawing 'E:\P2C Drive\_Belgard\_Details\01 ICP\z Details\Finals\DWG\S13 Belgard Std Paver Install Utility Str.dwg' refers to a cache manifest XML file, zero or more cache files (.GWS) as well as raw data files.

Please ensure the manifest XML file and cache files are unzipped to the drawing directory or your current MapCache directory.

You may also need to update the cache manifest XML file to point to the unzipped location of the data files.



